**RY-YH Twin-shaft pre-mixer**

**The main application and characteristics of the machine**

Twin shaft pre-mixer with the feature of high mixing speed, good uniformity, can be mixed with 30% moisture viscous materials, work with two rotating opposite paddle rotor stirring in the middle, due to the paddle has a special angle, regardless of the shape of the material, the size of the density of how, are able to quickly and effectively mixed, discharge speed, less residue.

**Technical parameters:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Specification Model | Rotor diameter (mm) | Production capacity (t/h) | Power (kw) | Weight (t) |
|  |  |  |  |  |

